

**Date: 3rd Jun 2020**

Christian Mission for Development (CMD) is a registered non-profit, non-governmental, multi-sectoral relief and development organization dedicated to fighting poverty and injustices; and to enhance provision of holistic social services to reduce human suffering. CMD was established in 2005 to equip people with skills and to facilitate relief and development assistance to communities in need with special focus on women, children and youth initiatives

**REQUEST FOR QUOTE**

**Deadline for submission of Quotation is 10th Jun 2020- by 05:00PM**

**Send to**:

Christian Mission for Development

Tongpiny plot 157 BK III 3RD, Class Residential Area

Next to Catholic University

Juba, South Sudan

OR

By Email:

[**cmdlogs@cmdafrica.org**](mailto:cmdlogs@cmdafrica.org)

**RFQ No: CMD/FSL-2020-02, Supply of storage PVC Tents for storage.**

Christian Mission for Development- CMD wishes to contract a legally recognized service provider (company) for the supply of PVC Tents for storage to CMD Juba as listed below: -


|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | **Specifications** | **Unit** | **Quantity** |
| 1. | **TPVC Tent – 3x4m**  General 3x4 Storage Tent / Shelter w. ground frame, PVC 500 g/m² white  * Fixing floor frame - flexibly removable if required * With tear-resistant patterned inner fabric * Bolted screw connection   **Materials and thicknesses**   |  |  | | --- | --- | | Roof tarpaulin: | approx. 500 g/m²; 100 % PVC |   Side panels: approx. 500 g/m²  Steel pipes: approx. 38 mm  Wall thickness of poles: approx. 1.2 mm  Steel pole connectors: approx. 42 mm  Wall thickness of connectors: approx. 1.4 mm  **Product sizes:**  Width: approx. 3.00 m  Length: approx. 4.00 m  Lateral height: approx. 2.00 m  Ridge height: approx. 2.9 m  Leg distance (for max. side entrance width): approx. 2 m  WxL gate 1: approx. 2.0 x 2.0 m  WxL gate 2: approx. 1.0 x 2.0 m  **Weather resistance:**  100% waterproof  UV-resistant:  UV sun protection factor:- 80+ | PC | 3 |

**See Photos:**

****

****


****

****

****

Diameter foot plate approx. 11 cm

****Bolts and screws

****With tear-resistant patterned inner fabric.

**Statement of compliance with Terms and conditions.**

|  |  |
| --- | --- |
| Delivery Terms | To be delivered to the specified location and delivery period to be specified |
| Payment Terms | Bank transfer/ Cheque |
| Validity of Quotation | 90 days |
| Currency of prize | USD |
| Location of delivery | Juba, CMD Office |
| Cost | All cost Inclusive up to delivery point(Juba) |
| Warranty and After sales requirement | Warranty and After - sales services, details to be indicated. Minimum -1-year warranty on both parts and labor.  Services unit to be provided when the purchased unit is under repair. |