|  |  |
| --- | --- |
| Engine Type | Air-cooled, 2-stroke, reed-valve, single |
| Displacement | 123 cm3 |
| Bore x stroke | 56.0 x 50.0 mm |
| Compression ratio | 7.2:1 |
| Maximum power | 11.0 kW (15.0 PS) @ 7,000 rpm |
| Maximum torque | 15.2 N·m (1.5 kgf·m) @ 6,500 rpm |
| Lubrication system | Separate lubrication |
| Fuel supply | Carburetor |
| Ignition system | C.D.I. |
| Starting system | Kick |
| Fuel tank capacity | 9.5 liters |
| Oil tank capacity | 0.9 liters \*2-stroke engine oil |
| Transmission type | Constant mesh 6-speed |
| Shift type | Return |

**HASSIS**

|  |  |
| --- | --- |
| Overall length | 2,110 mm |
| Overall width | 865 mm |
| Overall height | 1,165 mm |
| Seat height | 830 mm |
| Wheelbase | 1,340 mm |
| Ground clearance | 260 mm |
| Weight | 107 kg \*with oil and a full fuel tank |
| Front Suspension | Telescopic forks |
| Rear Suspension | Swingarm |
| Front Brake | Drum |
| Rear Brake | Drum |
| Front Tyre | 2.75-21 45P |
| Rear Tyre | 4.10-18 59P |

