**Malteser International**

**Country Coordination Office**

**Plot No: 445 Kololo Road 3k South**

**Tong Ping, Juba Town**

**South Sudan**

**11 March 2022**

**Request for Quotations**

**RFQ\_JUB\_2022\_0060\_A**

For rehabilitation of ten boreholes in Juba County in South Sudan

1. Annex 1: Specification of Tendering
2. Annex 2: Bill of Quantity

We look forward to receiving your tenders by or before the **submission deadline on 18 March 2022 at or before 4:00 pm** via E-mail to**:** [**mb.procurement-juba@malteser-international.org**](mailto:mb.procurement-juba@malteser-international.org).

Please write in the Subject line of your email with tender: **RFQ\_JUB-2022\_0060\_A for rehabilitation of ten boreholes in Juba County**

Thank you for your cooperation.

Sincerely Yours,

|  |  |  |
| --- | --- | --- |
| [Logo Malteser International](http://www.malteser-international.org/) |  | Nermin Silajdzic  Country Logistics and Security Cordinator  Plot No. 445, Block 3, Kololo - US Embassy Road.  Central Equitorial State, Juba, South Sudan M: +211 (0) 911 746 963 · M: +211 (0) 924 767 949 [nermin.silajdzic@malteser-international.org](mailto:nermin.silajdzic@malteser-international.org) · Skype: nsilajdzic [www.malteser-international.org](http://www.malteser-international.org/) Malteser International Europe/Malteser Hilfsdienst e. V., County Court Cologne, VR 4726 Executive Board: Karl Prinz zu Löwenstein, Dr. Elmar Pankau, Douglas Graf Saurma-Jeltsch, Verena Hölken |
|  |  | [icon facebook](https://www.facebook.com/malteserinternational) [icon youtube](https://www.youtube.com/user/MalteserInt) |
| Legal advice: This communication is for use by the intended recipient and contains information that may be privileged, confidential or copyrighted under applicable law. If you are not the intended recipient, you are hereby formally notified that any use, copying or distribution of this e-mail, in whole or in part, is strictly prohibited. Please notify the sender by return e-mail and delete this e-mail from your systems. | | |

 please consider the environment before printing this email

# A. SPECIFICATION OF BIIDING

Related to our advertised the Request for Quotations (RFQs) RFQ\_JUB\_2022\_0060\_A Malteser International (MI) herewith calls for rehabilitation of ten boreholes in Juba County in South Sudan.

Under the following reference number:

Donor project numbers: 1373-WAU

# Description of the organization and its activities

Malteser International, the worldwide relief agency of the Sovereign Order of Malta for humanitarian aid, has more than 50 years of experience in humanitarian relief and covers around 100 projects in some 20 countries in Africa, Asia and the Americas, annually. It provides aid in all parts of the world without distinction of religion, race or political persuasion. Christian values and the humanitarian principles of impartiality and independence are the foundation of its work.

In South Sudan, Malteser International operates in Juba, Yei, Wau and Uyujuku. In these locations, it’s activities include Health and Nutrition, Food Security and Livelihood, Water Sanitation and Hygiene and Health Programs

**Objective of RFQ:** In accordance with the overall targets of above-mentioned operations, MI plans to order tenders for rehabilitation of ten boreholes in Juba County in South Sudan.

The technical specifications and conditions of the tendering process are described below in the Specification of Tendering and in the Annex 2: Bill of Quantity which are part of this RfQ.

Suppliers are invited to present tenders complying with the requirements here below specified.

# Tender Presentation

The tender shall be via E-mail to**:** [**mb.procurement-juba@malteser-international.org**](mailto:mb.procurement-juba@malteser-international.org)

**The deadline for the delivery of the tenders** **is: 18 March 2022 at or before 4:00pm**

* The tender shall be written in English
* The tender should be valid for **60 days after the deadline**
* The format BoQ can be used or a separate one depending on supplier’s choice.

# General conditions

* The tender shall be typed or written and signed on each page by the legal representative of the supplier,
* The winning supplier might be requested to provide catalogues, pictures, technical descriptions and/or samples of items at the order stage when required,
* The prices of the tenders will be expressed in United States Dollars. The prices must be on unit price basis as well as by totals,
* The prices will be considered fixed. No additional change of whatsoever nature and type will be accepted by Malteser International,
* MI reserves the right to accept or reject all tenders depending on prevailing condition at the time.

# Technical specification

|  |  |  |  |
| --- | --- | --- | --- |
| No | Item Description | Unit | Quantity |
| 1.00 | Allow for dismantling and removal of damaged head assembly, Allow for provision and fix new Head assembly Indian MK II or M KIII , well fixed using MS 16mm bolts and nuts | Borehole | 10 |
| 2.00 | Allow for dismantling and removal of water tank assembly, hence provide and allow for fixing new ones using MS 16mm bolts and nuts | PCS | 10 |
| 3.00 | Dismantling and removal of damaged GI. Pipes 11/4''- 3 M complete with 12 mm connecting rods, hence provide and allow for fixing new ones in place | Set | 10 |
| 4.00 | Dismantling and removal of damaged/ depreciated Pedesntal assembly , hence provide and allow fixing new Indian MK II or Mark III Pedesntal in each borehole. | Set | 10 |
| 5.00 | Dismantling and removal of damaged/ depreciated cylinder assembly , hence provide and allow fixing new Indian MK II or Mark III Cylinder in each borehole. | PCS | 10 |
| 6.00 | Allow for dismantling damaged aprons, hence provide and allow for major repair of complete apron including drainage channels, allow for general Excavation of the top soil & cut away depth 200mm (assume 2.00m dia. And 6.00 long x 0.2m channel inclusive) | Borehole | 10 |
| 7.00 | Use Chlorination to disinfect all the borehole in actual calculated ratio | Borehole | 10 |
| 8.00 | Provision and casting of 1:2:3 reinforced concrete well compacted for the platform and apron, drainage channels and soak way pit including screening cement metal on the casted surfaces | Cu-m | 20 |
| 9.00 | Excavation for soak away pit & cart away 1x1x1.5 M with a provision of approved filling material in soak way pit including polythene sheeting cover | Cu-m | 20 |

# Validity of tenders

Each company is bound to the tender submitted for a period of 60 days from the deadline for submission of tenders.

# Language of tenders

All tenders, official correspondence between companies and MI, as well as all documents associated with the tender request will be in English.

# Submission of tenders

All tenders must conform to the following conditions:

# Each tender must submitted via E-mail to: [mb.procurement-juba@malteser-international.org](mailto:mb.procurement-juba@malteser-international.orga) on 18 March 2022, at or before 04:00 pm (local time).

# Content of tenders

All submitted tenders must conform to the requirements mentioned in the RFQ. Furthermore, they must include the following documents:

**Part 1 - Tender:** A tender for the bided rehabilitation of ten boreholes in Juba County in South Sudan. The format BoQ can be used or a separate one depending on supplier’s choice. Additional sheets may be attached for further details.

**Part 2 - Legal documents**

* Copy of the company’s certificate of incorporation,
* Copy of Chamber of Commerce registration,
* Copy Tax Identification Certificate,
* Copy of Certificate of Operation,
* Company’s Bank Statement of last three months,
* Company’s official address,
* Bank account details (where money would be paid),

# Ownership of tenders

MI reserves/funds ownership of all tender received. As a consequence, bidders will not be able to stipulate requirements that their tenders are to be returned.

1. **Opening of submitted tenders**

The tenders will be opened on 18 March 2022 in MI Country Coordination Office in Juba, South Sudan, by the Evaluation committee. The selection process will be recorded in writing by the committee.

# Tenders evaluation

The criteria applied for the evaluation will be the legal conformity, the price, the technical experiences, the compliance with technical specifications and quality standards, and the capacity to deliver, delivery time and meet timeframes as specified. The work will be awarded to the winning bidder according to the timetable mentioned above.

1. **Exclusion criteria**

**The following are exclusion criteria:**

1. **Not submitted the following company registration documents in South Sudan:**
   * 1. **Copy of the company’s certificate of incorporation,**
     2. **Copy of Chamber of Commerce registration,**
     3. **Copy Tax Identification Certificate,**
     4. **Copy of Certificate of Operation,**
2. **Not bided according to the specification and**
3. **Mathematical error of total bided price >±2 %.**
4. **Specific Technical and Financial Evaluation Criteria to standards:**

* Comparative Bid Analysis and justification basing on responsiveness of the selected supplier by evaluation committee.
* Contract agreement will directly be issued to the selected supplier upon approval.

1. **Terms of payment**

The payment will be done in United States Dollar by bank transfer or cheque as specified below:

* Payment terms will be within 10 business days after receipt of goods and invoice, by Electronic bank transfer.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Annex 2: Bill of Quantity** |  |  |  |  |

For rehabilitation of ten boreholes in Juba County in South Sudan

1- Liriya Primary School in Lirya Payam

2- Lokiliri Primary School in Lokiliri Payam, 3- Iliangari Primary School in Lirya Payam,

4- Ngangala Primary School in Lirya Payam, 5- Bori Primary School in Ladu Payam,

6- Don Bosco PHCC in Rajaf Payam,

7- Peiti PHCU in Northen Bari Payam,

8- Gudele PHCU in Munuki Payam,

9- Luri Rokwe PHCU in Northen Bari Payam

10- Lologo I PHCU/ Khor William PHCU in Kator Payam.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No | Item Description | Unit | Quantity | Unit rate USD | Amount USD |
| 1.00 | Allow for dismantling and removal of damaged head assembly, Allow for provision and fix new Head assembly Indian MK II or M KIII , well fixed using MS 16mm bolts and nuts | Borehole | 10 |  |  |
| 2.00 | Allow for dismantling and removal of water tank assembly, hence provide and allow for fixing new ones using MS 16mm bolts and nuts | PCS | 10 |  |  |
| 3.00 | Dismantling and removal of damaged GI. Pipes 11/4''- 3 M complete with 12 mm connecting rods, hence provide and allow for fixing new ones in place | Set | 10 |  |  |
| 4.00 | Dismantling and removal of damaged/ depreciated Pedesntal assembly , hence provide and allow fixing new Indian MK II or Mark III Pedesntal in each borehole. | Set | 10 |  |  |
| 5.00 | Dismantling and removal of damaged/ depreciated cylinder assembly , hence provide and allow fixing new Indian MK II or Mark III Cylinder in each borehole. | PCS | 10 |  |  |
| 6.00 | Allow for dismantling damaged aprons, hence provide and allow for major repair of complete apron including drainage channels, allow for general excavation of the top soil & cut away depth 200mm(assume 2.00m dia. And 6.00 long x 0.2m channel inclusive) | Borehole | 10 |  |  |
| 7.00 | Use Chlorination to disinfect all the borehole in actual calculated ratio | Borehole | 10 |  |  |
| 8.00 | Provision and casting of 1:2:3 reinforced concrete well compacted for the platform and apron, drainage channels and soak way pit including screening cement metal on the casted surfaces | Cu-m | 20 |  |  |
| 9.00 | Excavation for soak away pit & cart away 1x1x1.5 M with a provision of approved filling material in soak way pit including polythene sheeting cover | Cu-m | 20 |  |  |
|  | **Total for rehabilitation of ten boreholes** |  |  |  |  |

On behalf of Malteser International:

11 March 2022

Sincerely,

|  |  |  |
| --- | --- | --- |
| [Logo Malteser International](http://www.malteser-international.org/) |  | Nermin Silajdzic  Country Logistics and Security Coordinator Plot No. 445, Block 3, Kololo - US Embassy Road.  Central Equitorial State, Juba, South Sudan M: +211 (0) 911 746 963 · M: +211 (0) 924 767 949 [nermin.silajdzic@malteser-international.org](mailto:nermin.silajdzic@malteser-international.org) · Skype: nsilajdzic [www.malteser-international.org](http://www.malteser-international.org/) Malteser International Europe/Malteser Hilfsdienst e. V., County Court Cologne, VR 4726 Executive Board: Karl Prinz zu Löwenstein, Dr. Elmar Pankau, Douglas Graf Saurma-Jeltsch, Verena Hölken |
|  |  | [icon facebook](https://www.facebook.com/malteserinternational) [icon youtube](https://www.youtube.com/user/MalteserInt) |
| Legal advice: This communication is for use by the intended recipient and contains information that may be privileged, confidential or copyrighted under applicable law. If you are not the intended recipient, you are hereby formally notified that any use, copying or distribution of this e-mail, in whole or in part, is strictly prohibited. Please notify the sender by return e-mail and delete this e-mail from your systems. | | |

 please consider the environment before printing this email